Hinge Assembly

2. Insert the pin into the concentric cylinders to hold the hinges together.

1. Place the chromium hinges so that the cylinders are concentric.



