Helmet Assembly

2. Insert the black side lights into the press-fit whole in the side of the helmet.

1. Press fit the acrylic visor into the shell of the Mars helmet.



